|  |  |
| --- | --- |
| Model | ET2794L |
| Color | Black |
| Diagonal Size | 27” / 685.8 mm |
| Active Display Area | 23.53” x 13.23” / 597.6 x 336.15 mm |
| LCD Technology | Active matrix TFT LCD |
| Number of Touches | TouchPro PCAP: 10 Touches  IntelliTouch Dual Touch: 2 Touches  IntelliTouch/ IntelliTouch Zero-Bezel: Single Touch |
| Touch Technology | TouchPro PCAP, IntelliTouch Dual Touch, IntelliTouch, IntelliTouch Zero-Bezel |
| Aspect Ratio | 16:9 |
| Native Resolution | 1920x1080 |
| Preset Video Timings | 640x480 60Hz  720x400 70Hz  800x500, 60Hz  800x600 56, 60Hz  1024x768 60Hz  1280x800 60Hz  1280x1024 60Hz  1366x768 60Hz, 60Hz RB  1440x900 60Hz, 60Hz RB  1680x1050 60Hz, 60Hz RB  1920x1080 50, 60Hz |
| Number of Colors | 16.7 million |
| Brightness (typical) | **Panel:** 300 nits**; With IntelliTouch Zero-Bezel:** 270 nits; **With IntelliTouch:** 270 nits; **With IntelliTouch Dual:** 270 nits; **With TouchPro PCAP:** 270 nits; |
| Response Time (Tr + Tf) (typical) | 12 msec |
| Viewing Angle (typical) | **Horizontal:** ±89° / 178° total  **Vertical:** ±89° / 178° total |
| Contrast Ratio (typical) | 3000:1 |
| On-Screen Display (OSD) | Accessible through switches on the unit’s tethered OSD Control box.  **Controls**: Menu, Up, Down, Select, Power  **Settings**: Brightness, Contrast, Clock, Phase, H-Position, V-Position, Auto-Adjust, Aspect Ratio, Sharpness, Color Temperature, OSD Timeout, OSD Language, OSD H-Position, OSD V-Position, Recall Defaults, Video Priority, Information, Touch On Sleep Mode, Touch Through (Only available for TouchPro PCAP with E707022)  **Languages**: English, French, Italian, German, Spanish, Simplified Chinese, Traditional Chinese, Japanese,  **Lockouts**: OSD, Power |
| Mounting Options | 200x100mm VESA mount on rear of unit  4 Hole mounting interface on all four sides. Front mount with optional bezel kit (IntelliTouch/IntelliTouch Dual Touch Models see Accessories tab for details)  Flush mount with included brackets (TouchPro PCAP/IntelliTouch Zero-Bezel see dimensional drawings for details)  See dimensional drawings for details |
| I/O Ports | Serial port (Only available for IntelliTouch Zero-Bezel and IntelliTouch), USB TypeB, RJ45 for OSD remote key, VGA, HDMI, DisplayPort, 12V D/C in |
| Video | HDMI V1.3 Type A receptacle for HDMI input  Analog VGA on Female DB-15 connector  DisplayPort V1.1a - Supports later versions of DisplayPort video input  **Input Video Horizontal Sync frequency range:** 30 – 82K KHz  **Input Video Vertical Sync (frame rate) frequency range:** 50-75Hz |
| Power | **External DC - Optional power brick (sold separately)**  **Monitor input power connector: Coaxial power jack (2.0mm (+0.0 -0.1mm) pin outer diameter, 6.4mm (+/- 0.3mm) barrel inner diameter, 8.8mm (+/- 0.3mm) Barrel depth)**  **Monitor input voltage range: 12VDC +/- 5%**  **Adapter output power connector: DC barrel plug (2.1mm (+/- 0.1mm) pin inner diameter, 5.5mm (+/- 0.05mm) barrel outer diameter, 9.5mm (+/- 0.3mm) Barrel length)**  **Adapter input voltage range: 100-240 VAC**  **Input frequency: 50-60 Hz**  **Power Consumption (Typical):**  ON (monitor + adapter): 27W  SLEEP FROM PC (monitor + adapter): 1.5W  OFF (monitor + adapter): 0.5W |
| Audio | **N/A** |
| Weight | **Unpackaged:** 16.1 lbs. / 7.3 **k**g  **Packaged:** 22.49 lbs. / 10.2 kg |
| Dimensions (H x W x D) | **Unpackaged:**  IntelliTouch: 24.93” x 14.74” x 1.65” / 633.2 x 374.4 x 41.8 mm  IntelliTouch Dual Touch: 24.93” x 14.74” x 1.65” / 633.2 x 374.4 x 41.8 mm  IntelliTouch Zero-Bezel: 25.36” x 15.29” x 1.56” / 644.2 x 388.4 x 39.6 mm  TouchPro PCAP: 25.36” x 15.29” x 1.56” / 644.2 x 388.4 x 39.6 mm  **Packaged:** 30.79” x 20.87” x 7.87” / 782 x 530 x 200 mm |
| Temperature | **Operating:** 0° C to 40° C / 32° F to 104° F  **Storage:** -20° C to 60° C / -4° F to 140° F |
| Humidity (non-condensing) | **Operating:** 20% - 80%  **Storage:** 10% - 95% |
| Regulatory approvals and declarations | Australia RCM  Canada cUL, IC  China CCC  Europe CE, TUV  Japan VCCI  Korea KCC  Mexico CoC  Taiwan BSMI  United States UL, FCC  International CB  RoHS, China RoHS, WEEE |
| Compliance | GLI 27 kV air / 8 kV contact ESD compliant (TouchPro PCAP only)  UL 60950 ball-drop compliant (TouchPro PCAP only)  IK07 impact compliant (TouchPro PCAP only) |
| Warranty | 3 years |
| Additional Service Offerings |  |
| Extended Warranty | Elo P/N: E188404 – 1-year extended warranty  Elo P/N: E572038 – 2-year extended warranty |
| Other Features |  |
| Sealing |  |
| MTBF | 50,000 hours demonstrated |
| Box contents | HDMI cable  Touch USB Cable  VGA Cable  Remote OSD  Flush Mount Brackets w/Screws (TouchPro PCAP/IntelliTouch Zero-Bezel)  “L” (Side Mount) Brackets w/Screws (IntelliTouch/IntelliTouch Dual Touch Models)  Quick Install Guide  EEI Label  Japan Class-B TM info sheet |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Part Number | Part Description | Touch Technology | Surface Treatment | Touch Interface | Color |
| E335488 | ET2794L-4CWB-0-ST-ZB-NPB-G | IntelliTouch Zero-Bezel | Clear | Dual serial/USB2.0 | Black |
| E329077 | ET2794L-8UWB-0-DT-NPB-G | IntelliTouch Dual Touch | Clear | USB2.0 | Black |
| E329262 | ET2794L-8CWB-0-ST-NPB-G | IntelliTouch | Clear | Dual serial/USB2.0 | Black |
| E707022 | ET2794L-2UWC-0-MT-ZB-NPB-G | TouchPro PCAP | Clear | USB2.0 | Black |
|  |  |  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Options/Peripheral/Upgrades** | **Part #** | **Options/Peripheral/Upgrades** | **Part #** |
| ELO-REMOTE-OSD-RJ45-R | E483757 | ELO-PWR-BRICKCAB-LVL6-AU12V, 4.16A,50W-R | E637593 |
| REPLACEMENT CABLE KIT for 90 Series | E546861 | ELO-KIT-CABLE-DP-to-DP | E582895 |
| ELO-PWR-BRICKCAB-LVL6-NA12V, 4.16A, 50W-R | E005277 | Elo Backpack™ | E611864 |
| ELO-PWR-BRICKCAB-LVL6-EU-KR-12V, 50W-R | E571601 |  |  |
| ELO-PWR-BRICKCAB- LVL6-UK12V, 4.16A, 50W-R | E180092 |  |  |
| ELO-PWR-BRICKCAB- LVL6-CH12V, 4.16A, 50W-R | E558862 |  |  |
| ELO-PWR-BRICKCAB- LVL6-TW12V, 4.16A, 50W-R | E818655 |  |  |
| ELO-PWR-BRICKCAB- LVL6-JP12V, 4.16A, 50W-R | E182546 |  |  |
| ELO-PWR-BRICKCAB- LVL6-AR12V, 4.16A, 50W-R | E887099 |  |  |
| IntelliTouch Stylus Pen | D82064-000 |  |  |
| ELO-27INCHWIDE-L-BKT-R | E646994 |  |  |
| ELO-27INCHWIDE-FLUSHMOUNT-BKT-R | E190896 |  |  |
| ELO-27INCHWIDE-FRONTMOUNT-BEZ-R | E589935 |  |  |
| ELO-KIT-CABLE-DVI-D-to-HDMI | E538507 |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |
| --- | --- |
| Document Number | Description |
| E893866 | QIG |
| MS601696 | Dimensional drawings ET2794L |
| MD600070 | Regulatory certificates |
| UM600129 | User Guide – English |
| UM600130 | User Guide – French |
| UM600131 | User Guide – Italian |
| UM600132 | User Guide – German |
| UM600133 | User Guide – Spanish |
| UM600134 | User Guide – Japanese |
| UM600135 | User Guide – Simplified Chinese |
| UM600136 | User Guide – Traditional Chinese |
| UM600137 | User Guide – Korean |
| UM600138 | User Guide – Russian |

## ****MTBF (Mean Time Between Failures)**** An MTBF measurement is based on a statistical sample and is not intended to predict any one specific unit's reliability; thus, MTBF is not, and should not be construed as, a warranty measurement.